; ************************************************************
; ************************************************************
; **  Filename: AlderLakePCH-SSystem.inf                    **
; **  Abstract: Assigns the null driver to devices          **
; **            for yellow-bang removal and                 **
; **            brands Intel(R) devices                     ** 
; ************************************************************
; ************************************************************

[Version]
Signature=$WINDOWS NT$
Class=System
ClassGUID={4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider=%INTEL%
CatalogFile=AlderLakePCH-S.cat
DriverVer=07/18/1968, 10.1.37.7
PnpLockDown=1

[SourceDisksNames]

[SourceDisksFiles]

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%INTEL%=INTEL,NTx86,NTamd64

[INTEL.NTx86]
%PCI\VEN_8086&DEV_7A80Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A80
%PCI\VEN_8086&DEV_7A81Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A81
%PCI\VEN_8086&DEV_7A82Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A82
%PCI\VEN_8086&DEV_7A83Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A83
%PCI\VEN_8086&DEV_7A84Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A84
%PCI\VEN_8086&DEV_7A85Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A85
%PCI\VEN_8086&DEV_7A86Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A86
%PCI\VEN_8086&DEV_7A87Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A87
%PCI\VEN_8086&DEV_7A88Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A88
%PCI\VEN_8086&DEV_7A8ADesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A8A
%PCI\VEN_8086&DEV_7A8BDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A8B
%PCI\VEN_8086&DEV_7A8CDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A8C
%PCI\VEN_8086&DEV_7A8DDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A8D
%PCI\VEN_8086&DEV_7A8EDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A8E
%PCI\VEN_8086&DEV_7A8FDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A8F
%PCI\VEN_8086&DEV_7A90Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A90
%PCI\VEN_8086&DEV_7A91Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A91
%PCI\VEN_8086&DEV_7A92Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A92
%PCI\VEN_8086&DEV_7A93Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A93
%PCI\VEN_8086&DEV_7A94Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A94
%PCI\VEN_8086&DEV_7A95Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A95
%PCI\VEN_8086&DEV_7A96Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A96
%PCI\VEN_8086&DEV_7A97Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A97
%PCI\VEN_8086&DEV_7A98Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A98
%PCI\VEN_8086&DEV_7A99Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A99
%PCI\VEN_8086&DEV_7A9ADesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A9A
%PCI\VEN_8086&DEV_7A9BDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A9B
%PCI\VEN_8086&DEV_7A9CDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A9C
%PCI\VEN_8086&DEV_7A9DDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A9D
%PCI\VEN_8086&DEV_7A9EDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A9E
%PCI\VEN_8086&DEV_7A9FDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A9F
%PCI\VEN_8086&DEV_7AB0Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB0
%PCI\VEN_8086&DEV_7AB1Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB1
%PCI\VEN_8086&DEV_7AB2Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB2
%PCI\VEN_8086&DEV_7AB3Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB3
%PCI\VEN_8086&DEV_7AB4Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB4
%PCI\VEN_8086&DEV_7AB5Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB5
%PCI\VEN_8086&DEV_7AB6Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB6
%PCI\VEN_8086&DEV_7AB7Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB7
%PCI\VEN_8086&DEV_7AB8Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB8
%PCI\VEN_8086&DEV_7AB9Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB9
%PCI\VEN_8086&DEV_7ABADesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ABA
%PCI\VEN_8086&DEV_7ABBDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ABB
%PCI\VEN_8086&DEV_7ABCDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ABC
%PCI\VEN_8086&DEV_7ABDDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ABD
%PCI\VEN_8086&DEV_7ABEDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ABE
%PCI\VEN_8086&DEV_7ABFDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ABF
%PCI\VEN_8086&DEV_7AC0Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC0
%PCI\VEN_8086&DEV_7AC1Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC1
%PCI\VEN_8086&DEV_7AC2Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC2
%PCI\VEN_8086&DEV_7AC3Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC3
%PCI\VEN_8086&DEV_7AC4Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC4
%PCI\VEN_8086&DEV_7AC5Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC5
%PCI\VEN_8086&DEV_7AC6Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC6
%PCI\VEN_8086&DEV_7AC7Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC7
%PCI\VEN_8086&DEV_7AC8Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC8
%PCI\VEN_8086&DEV_7AC9Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC9
%PCI\VEN_8086&DEV_7ACADesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ACA
%PCI\VEN_8086&DEV_7ACBDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ACB
%PCI\VEN_8086&DEV_7AAFDesc%=Needs_NO_DRV,PCI\VEN_8086&DEV_7AAF
%PCI\VEN_8086&DEV_7AA0Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_7AA0
%PCI\VEN_8086&DEV_7AA1Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_7AA1
%PCI\VEN_8086&DEV_7AA7Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_7AA7
%PCI\VEN_8086&DEV_7AA3Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_7AA3
%PCI\VEN_8086&DEV_7AA4Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_7AA4

[INTEL.NTamd64]
%PCI\VEN_8086&DEV_7A80Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A80
%PCI\VEN_8086&DEV_7A81Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A81
%PCI\VEN_8086&DEV_7A82Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A82
%PCI\VEN_8086&DEV_7A83Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A83
%PCI\VEN_8086&DEV_7A84Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A84
%PCI\VEN_8086&DEV_7A85Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A85
%PCI\VEN_8086&DEV_7A86Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A86
%PCI\VEN_8086&DEV_7A87Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A87
%PCI\VEN_8086&DEV_7A88Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A88
%PCI\VEN_8086&DEV_7A8ADesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A8A
%PCI\VEN_8086&DEV_7A8BDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A8B
%PCI\VEN_8086&DEV_7A8CDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A8C
%PCI\VEN_8086&DEV_7A8DDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A8D
%PCI\VEN_8086&DEV_7A8EDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A8E
%PCI\VEN_8086&DEV_7A8FDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A8F
%PCI\VEN_8086&DEV_7A90Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A90
%PCI\VEN_8086&DEV_7A91Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A91
%PCI\VEN_8086&DEV_7A92Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A92
%PCI\VEN_8086&DEV_7A93Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A93
%PCI\VEN_8086&DEV_7A94Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A94
%PCI\VEN_8086&DEV_7A95Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A95
%PCI\VEN_8086&DEV_7A96Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A96
%PCI\VEN_8086&DEV_7A97Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A97
%PCI\VEN_8086&DEV_7A98Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A98
%PCI\VEN_8086&DEV_7A99Desc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A99
%PCI\VEN_8086&DEV_7A9ADesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A9A
%PCI\VEN_8086&DEV_7A9BDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A9B
%PCI\VEN_8086&DEV_7A9CDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A9C
%PCI\VEN_8086&DEV_7A9DDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A9D
%PCI\VEN_8086&DEV_7A9EDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A9E
%PCI\VEN_8086&DEV_7A9FDesc%=Needs_MSISADRV,PCI\VEN_8086&DEV_7A9F
%PCI\VEN_8086&DEV_7AB0Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB0
%PCI\VEN_8086&DEV_7AB1Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB1
%PCI\VEN_8086&DEV_7AB2Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB2
%PCI\VEN_8086&DEV_7AB3Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB3
%PCI\VEN_8086&DEV_7AB4Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB4
%PCI\VEN_8086&DEV_7AB5Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB5
%PCI\VEN_8086&DEV_7AB6Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB6
%PCI\VEN_8086&DEV_7AB7Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB7
%PCI\VEN_8086&DEV_7AB8Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB8
%PCI\VEN_8086&DEV_7AB9Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AB9
%PCI\VEN_8086&DEV_7ABADesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ABA
%PCI\VEN_8086&DEV_7ABBDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ABB
%PCI\VEN_8086&DEV_7ABCDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ABC
%PCI\VEN_8086&DEV_7ABDDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ABD
%PCI\VEN_8086&DEV_7ABEDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ABE
%PCI\VEN_8086&DEV_7ABFDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ABF
%PCI\VEN_8086&DEV_7AC0Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC0
%PCI\VEN_8086&DEV_7AC1Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC1
%PCI\VEN_8086&DEV_7AC2Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC2
%PCI\VEN_8086&DEV_7AC3Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC3
%PCI\VEN_8086&DEV_7AC4Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC4
%PCI\VEN_8086&DEV_7AC5Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC5
%PCI\VEN_8086&DEV_7AC6Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC6
%PCI\VEN_8086&DEV_7AC7Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC7
%PCI\VEN_8086&DEV_7AC8Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC8
%PCI\VEN_8086&DEV_7AC9Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7AC9
%PCI\VEN_8086&DEV_7ACADesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ACA
%PCI\VEN_8086&DEV_7ACBDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_7ACB
%PCI\VEN_8086&DEV_7AAFDesc%=Needs_NO_DRV,PCI\VEN_8086&DEV_7AAF
%PCI\VEN_8086&DEV_7AA0Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_7AA0
%PCI\VEN_8086&DEV_7AA1Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_7AA1
%PCI\VEN_8086&DEV_7AA7Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_7AA7
%PCI\VEN_8086&DEV_7AA3Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_7AA3
%PCI\VEN_8086&DEV_7AA4Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_7AA4

[Needs_MSISADRV]
Include=machine.inf
Needs=MSISADRV

[Needs_MSISADRV.Services]
Include=machine.inf
Needs=MSISADRV.Services

[Needs_PCI_DRV]
Include=machine.inf
Needs=PCI_DRV

[Needs_PCI_DRV.Services]
Include=machine.inf
Needs=PCI_DRV.Services

[Needs_PCI_DRV.HW]
Include=machine.inf
Needs=PCI_DRV.HW

[Needs_NO_DRV]
Include=machine.inf
Needs=NO_DRV

[Needs_NO_DRV.Services]
Include=machine.inf
Needs=NO_DRV.Services

[Strings]
INTEL="INTEL"
PCI\VEN_8086&DEV_7A80Desc="Intel(R) LPC Controller/eSPI Controller - 7A80"
PCI\VEN_8086&DEV_7A81Desc="Intel(R) LPC Controller/eSPI Controller (SuperSKU unlocked) - 7A81"
PCI\VEN_8086&DEV_7A82Desc="Intel(R) LPC Controller/eSPI Controller (SuperSKU locked) - 7A82"
PCI\VEN_8086&DEV_7A83Desc="Intel(R) LPC Controller/eSPI Controller (Q670) - 7A83"
PCI\VEN_8086&DEV_7A84Desc="Intel(R) LPC Controller/eSPI Controller (Z690) - 7A84"
PCI\VEN_8086&DEV_7A85Desc="Intel(R) LPC Controller/eSPI Controller (H670) - 7A85"
PCI\VEN_8086&DEV_7A86Desc="Intel(R) LPC Controller/eSPI Controller (B660) - 7A86"
PCI\VEN_8086&DEV_7A87Desc="Intel(R) LPC Controller/eSPI Controller (H610) - 7A87"
PCI\VEN_8086&DEV_7A88Desc="Intel(R) LPC Controller/eSPI Controller (W680) - 7A88"
PCI\VEN_8086&DEV_7A8ADesc="Intel(R) LPC Controller/eSPI Controller (W790) - 7A8A"
PCI\VEN_8086&DEV_7A8BDesc="Intel(R) LPC Controller/eSPI Controller (SuperSKU Locked) - 7A8B"
PCI\VEN_8086&DEV_7A8CDesc="Intel(R) LPC Controller/eSPI Controller - 7A8C"
PCI\VEN_8086&DEV_7A8DDesc="Intel(R) LPC Controller/eSPI Controller - 7A8D"
PCI\VEN_8086&DEV_7A8EDesc="Intel(R) LPC Controller/eSPI Controller - 7A8E"
PCI\VEN_8086&DEV_7A8FDesc="Intel(R) LPC Controller/eSPI Controller - 7A8F"
PCI\VEN_8086&DEV_7A90Desc="Intel(R) LPC Controller/eSPI Controller (R680E) - 7A90"
PCI\VEN_8086&DEV_7A91Desc="Intel(R) LPC Controller/eSPI Controller (Q670E) - 7A91"
PCI\VEN_8086&DEV_7A92Desc="Intel(R) LPC Controller/eSPI Controller (H610E) - 7A92"
PCI\VEN_8086&DEV_7A93Desc="Intel(R) LPC Controller/eSPI Controller - 7A93"
PCI\VEN_8086&DEV_7A94Desc="Intel(R) LPC Controller/eSPI Controller - 7A94"
PCI\VEN_8086&DEV_7A95Desc="Intel(R) LPC Controller/eSPI Controller - 7A95"
PCI\VEN_8086&DEV_7A96Desc="Intel(R) LPC Controller/eSPI Controller - 7A96"
PCI\VEN_8086&DEV_7A97Desc="Intel(R) LPC Controller/eSPI Controller - 7A97"
PCI\VEN_8086&DEV_7A98Desc="Intel(R) LPC Controller/eSPI Controller - 7A98"
PCI\VEN_8086&DEV_7A99Desc="Intel(R) LPC Controller/eSPI Controller - 7A99"
PCI\VEN_8086&DEV_7A9ADesc="Intel(R) LPC Controller/eSPI Controller - 7A9A"
PCI\VEN_8086&DEV_7A9BDesc="Intel(R) LPC Controller/eSPI Controller - 7A9B"
PCI\VEN_8086&DEV_7A9CDesc="Intel(R) LPC Controller/eSPI Controller - 7A9C"
PCI\VEN_8086&DEV_7A9DDesc="Intel(R) LPC Controller/eSPI Controller - 7A9D"
PCI\VEN_8086&DEV_7A9EDesc="Intel(R) LPC Controller/eSPI Controller - 7A9E"
PCI\VEN_8086&DEV_7A9FDesc="Intel(R) LPC Controller/eSPI Controller - 7A9F"
PCI\VEN_8086&DEV_7AB0Desc="Intel(R) PCI Express Root Port #9 - 7AB0"
PCI\VEN_8086&DEV_7AB1Desc="Intel(R) PCI Express Root Port #10 - 7AB1"
PCI\VEN_8086&DEV_7AB2Desc="Intel(R) PCI Express Root Port #11 - 7AB2"
PCI\VEN_8086&DEV_7AB3Desc="Intel(R) PCI Express Root Port #12 - 7AB3"
PCI\VEN_8086&DEV_7AB4Desc="Intel(R) PCI Express Root Port #13 - 7AB4"
PCI\VEN_8086&DEV_7AB5Desc="Intel(R) PCI Express Root Port #14 - 7AB5"
PCI\VEN_8086&DEV_7AB6Desc="Intel(R) PCI Express Root Port #15 - 7AB6"
PCI\VEN_8086&DEV_7AB7Desc="Intel(R) PCI Express Root Port #16 - 7AB7"
PCI\VEN_8086&DEV_7AB8Desc="Intel(R) PCI Express Root Port #1 - 7AB8"
PCI\VEN_8086&DEV_7AB9Desc="Intel(R) PCI Express Root Port #2 - 7AB9"
PCI\VEN_8086&DEV_7ABADesc="Intel(R) PCI Express Root Port #3 - 7ABA"
PCI\VEN_8086&DEV_7ABBDesc="Intel(R) PCI Express Root Port #4 - 7ABB"
PCI\VEN_8086&DEV_7ABCDesc="Intel(R) PCI Express Root Port #5 - 7ABC"
PCI\VEN_8086&DEV_7ABDDesc="Intel(R) PCI Express Root Port #6 - 7ABD"
PCI\VEN_8086&DEV_7ABEDesc="Intel(R) PCI Express Root Port #7 - 7ABE"
PCI\VEN_8086&DEV_7ABFDesc="Intel(R) PCI Express Root Port #8 - 7ABF"
PCI\VEN_8086&DEV_7AC0Desc="Intel(R) PCI Express Root Port #17 - 7AC0"
PCI\VEN_8086&DEV_7AC1Desc="Intel(R) PCI Express Root Port #18 - 7AC1"
PCI\VEN_8086&DEV_7AC2Desc="Intel(R) PCI Express Root Port #19 - 7AC2"
PCI\VEN_8086&DEV_7AC3Desc="Intel(R) PCI Express Root Port #20 - 7AC3"
PCI\VEN_8086&DEV_7AC4Desc="Intel(R) PCI Express Root Port #21 - 7AC4"
PCI\VEN_8086&DEV_7AC5Desc="Intel(R) PCI Express Root Port #22 - 7AC5"
PCI\VEN_8086&DEV_7AC6Desc="Intel(R) PCI Express Root Port #23 - 7AC6"
PCI\VEN_8086&DEV_7AC7Desc="Intel(R) PCI Express Root Port #24 - 7AC7"
PCI\VEN_8086&DEV_7AC8Desc="Intel(R) PCI Express Root Port #25 - 7AC8"
PCI\VEN_8086&DEV_7AC9Desc="Intel(R) PCI Express Root Port #26 - 7AC9"
PCI\VEN_8086&DEV_7ACADesc="Intel(R) PCI Express Root Port #27 - 7ACA"
PCI\VEN_8086&DEV_7ACBDesc="Intel(R) PCI Express Root Port #28 - 7ACB"
PCI\VEN_8086&DEV_7AAFDesc="Intel(R) IEH - 7AAF"
PCI\VEN_8086&DEV_7AA0Desc="Intel(R) P2SB - 7AA0"
PCI\VEN_8086&DEV_7AA1Desc="Intel(R) PMC - 7AA1"
PCI\VEN_8086&DEV_7AA7Desc="Intel(R) Shared SRAM - 7AA7"
PCI\VEN_8086&DEV_7AA3Desc="Intel(R) SMBus - 7AA3"
PCI\VEN_8086&DEV_7AA4Desc="Intel(R) SPI (flash) Controller - 7AA4"




; Copyright (c) 2003-2019 Intel Corporation
; 
; ********************************************************************************
; Intel is making no claims of usability, efficacy or warranty.
; ********************************************************************************
; Information in this document is provided in connection with Intel products. No
; license, express or implied, by estoppel or otherwise, to any intellectual
; property rights is granted by this document. Intel assumes no liability
; whatsoever, and Intel disclaims any express or implied warranty, relating to
; sale and/or use of Intel products including liability or warranties relating to
; fitness for a particular purpose, merchantability, or infringement of any
; patent, copyright or other intellectual property right. Intel products are not
; intended for use in medical, life saving, or life sustaining applications.
; ********************************************************************************
; Intel Corporation disclaims all warranties and liabilities for the use of this
; document and the information contained herein, and assumes no responsibility for
; any errors which may appear in this document, nor does Intel make a commitment
; to update the information contained herein. Intel reserves the right to make
; changes to this document at any time, without notice.
; ********************************************************************************
; ********************************************************************************
; 
; * Third-party brands and names are the property of their respective owners.
